HID touch screen driver installation for Fedora Core 5 and X11 
(C) 2006 Chang-Hsieh Wu

==============================================================================
QUICKSTART GUIDE
==============================================================================
1. setup xfree driver
   a. decompress xfhiddrv_drv.tar.gz
      #gzip -d xfhiddrv_drv.tar.gz
      #tar xvf xfhiddrv_drv.tar 
   b. Copy xfhiddrv_drv.o to /usr/lib/xorg/modules/input/xfhiddrv_drv.so or other place where 
      your X is installed.
      #cp   xfhiddrv_drv.o /usr/lib/xorg/modules/input/xfhiddrv_drv.so
   c. Add the following lines into xorg.conf(maybe in /etc or /etc/X11)file.
      If your system will not have a mouse, then use "CorePointer" instead of
      "SendCoreEvents" in the "ServerLayout" section.  Set "ServerLayout"  section
      as the following.

#	InputDevice    "DevInputMice" "AlwaysCore"
    	InputDevice 	"Touchscreen0" "SendCoreEvents"


   d. Add the a new "InputDevice" Section as the following.
Section "InputDevice"
        Identifier  "Touchscreen0"
        Driver      "xfhiddrv"
        Option      "Device" "/dev/hiddev0"
        Option      "ScreenNo" "0"
        Option      "Rotation" "0"
        Option      "SwapY" "0"
        Option      "DebugLevel" "0"
        Option      "AlwaysCore"
        Option      "UpSound" "1"
        Option      "DownSound" "1"
        Option      "AutoRightClick" "1"
        Option      "TouchMode" "2"
EndSection

    In the item of "Device", you must depend on your computer. So, it can be the value, 
such as the followings.
        "/dev/hiddevx"  x=0,1,..2, n

   e. Press Ctrl+Alt+Backspace to restart X server. 

2. Setup and run Linear Utility:
   I. Linearity Utility:
   a. installation 
      step 1. decompress LinearAp.tar.gz 
         #gzip -d LinearAp.tar.gz
         #tar xvf LinearAp.tar.gz 
      step 2. copy linearity utility to /usr/local/bin
         #cp ./LinearAp /usr/local/bin
   b. Run linearity utility
      I. HID device
      #./LinearAp  /dev/hiddevx n
      II. RS232 device
      #./LinearAp  /dev/ttySx n
      where x=0,1,2...n, n = 4 or 9 <default>  
      
      
